FC-102P7K5T4E21H2XGX1XXSXXXXAGBXCXXXXDX

131N2581

Frequency Converter

FC-102P7K5T4E21H2XGX1XXSXXXXAGBXCXXXXDX

VLT® HVAC Drive FC-102

(P7K5) 7.5 KW / 10 HP, Three phase

380 - 480 VAC, IP21 / Type 1

RFI Filter

No brake chopper

Graphical Loc. Cont. Panel

Not coated PCB, Mains Disconnect

Latest release std. SW.

LonWorks MCA 108, No B Option

No C1 option, No D option

Frame: A3

Other options according to Model Code

Model code:

FC-102P7K5T4E21H2XGX1XXSXXXXAGBXCXXXXDX