MCD202015T6CV3

VLT® Compact Starter MCD 202

15 kW 34A:4-6: 354

Three phase, 200-575 VAC

Control voltage: 110/240 VAC or 440 VAC

1. A-Frame

Product Group MCD VLT® Soft Starter MCD

MCD Series 202 202

Power Rating 015 15 kW 34A:4-6: 354

Phase T Three phase

Mains Voltage 6 200-575 VAC

Control Supply Voltage CV3 110/240 VAC or 440 VAC

Frame Size A (A) A-Frame

Typecode Part 1 MCD202015T6CV3

Product Catalog NO\_VIEW NO VIEW

Modelcode01 MCD202015T6CV3